Start Up Procedure for Propane Grinders:

1. Turn on Gas
2. Increase throttle slightly
3. Turn key
4. Once motor turns over, increase throttle until the motor is running around 2,500 rpms
5. Push the “engagement” switch
6. Immediately begin swinging left to right.

When ready to stop

1. Decrease throttle to 1,200 rpms
2. Turn off gas
3. Continue swinging machine side to side until the motor dies and the operator is unable to move it anymore.
4. Turn the key to the off position