

***The Novair F2105***

**"The complete package!"** Our most powerful, durable & light weight Negative Air Machine available! ***Virtually Indestructible!***

**FEATURES AND BENEFITS:**• Powerful 2HP motor generates exceptional, consistent flow rate and utilizes all filter media area
• 2 speed motor-provides consistent air flow of 2000cfm (high speed) and 1000cfm (low speed)
• 8 point motor/cage mounting prevents motor and cage shifting under the harshest conditions
• Seamless construction guarantees leak proof operation
• One of the lightest 2000cfm units on the market is easily transported by 2 operators
• Positive lock filter prevents filter movement for uninterrupted filtration
• Uses standard 24" x 24" H.E.P.A. filters, rated 99.97% efficiency against 0.3 micron particles
• General Purpose Filters & Audible Alarms are also available
• Custom controls & features available upon request

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| F2105 | 118lbs | 37" x 26" x 31" | 2HP-Two Speed, Thermally Protected | High-2000cfmLow-1200cfm | 115Volt15 Amp, 60Hz | 1/2" Pad / Ring Filter |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ring | Pad |  | door | hepa |
|  **Ring FiltersPart No: 55014** | **Pad FilterPart No: 55007** |  | **12" Vacuum Intake DoorPart No: A31091** | **General Purpose Filter KitPart No: A30176****Replacement General Filter Only:** **A40023** |